**LOT 6: Supply of Poultry Farm Equipment and Materials to the Integrated Polytechnic Regional College (IPRC) Gishari.**

*Bidders are expected to examine carefully and comply with all instructions and specifications.*

**Date: \_\_\_\_\_\_/\_\_\_\_\_\_/\_\_\_\_\_\_\_\_\_**

**Bidder Information**

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
| Bidder’s Legal Name |  |  |
|  |
| TIN Number |  |  |
|  |  |  |
| Country/ies of Registration/Operation |  |  |
|

|  |
| --- |
|  |

Bidder’s Authorized Representative |
|  |  |  |  |  |
| Title |  |  Telephone |  |  |
|  |
| Email |  |  |
|  |

**Descriptions and Specifications of Poultry Farm Equipment and Materials to be supplied to IPRC Gishari.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **No.** | **Item Description** | **Item Specifications** | **Units** | **Quantity** | **Unit Price (Frw)** | **Total Price (Frw)** |
|  | Cages for layers  | Galvanised steel meshed Cells length=430mm, cell depth=420mm, cell height=410mm, tier/set=4, birds per cell/unit/set=4/20/160 with semi-automatic drinking system and automatic manure removal system with galvanized steel stands | Set | 2 |  |  |
|  | Spades | Shovel, round point with Y handle, total length approx.1m | Pc | 2 |  |  |
|  | Fork Hoes  | Hoe Head: Width = 18cm, Height = 26cm, Thickness = 3/8" | Pc | 2 |  |  |
|  | Sheeting  | Plastic sheets 7mx8m | Pc | 6 |  |  |
|  | Thermometer  | Product size: 210mm X 55mm, Product material: ABS plastic shell, Accurate measurement: temperature +/-1℃, Temperature range: -15℃-50℃, Method of use: hanging | Pc | 2 |  |  |
|  | Electronic balance  | Electronic scale, with capacity of 30kg to 600 kg, Painted steel scale, with LCD display, check weighing with LED indication, Reading unit with 52 mm backlit LCD display and 7 command key, -Power: AC adapter (12V/500mA) | Pc | 2 |  |  |
|  | Sprayer pump | Hand operated knapsack sprayer 20liters capacity | Pc | 4 |  |  |
|  | Charcoal stoves  | Charcoal briquettes for chicken brooding, ceramic type | Pc | 6 |  |  |
|  | Incubator  | Automatic egg incubator with Temperature Range= +8°C above ambient to 80°C, Chamber Dimensions (WxDxH)= (93 x 106 x 168) cm, Power Requirements=120VAC, 50/60Hz, single phase (220V available), Digital control and digital display with soak timer | Pc | 2 |  |  |
|  | Heaters/brooders  | Infra-Red Heat Lamp Holder With 250 Watt Bulb for Poultry | Pc | 4 |  |  |
|  | Wheelbarrows  | Galvanised Steel Tubular Frame, Body Weight Capacity of 100kgs 30cm dia-wheel, External Pan Measurements:53/59(W) x 85(L) 22cm(H) | Pc | 2 |  |  |
|  | Drinkers  | Drinker Type=Pan and Jar, Capacity (Ltrs)3 Litre, White Colour and Red, Material Plastic, Thickness 2.6-5.5 mm, Pan Diameter357 mm | Pc | 10 |  |  |
|  | Feeders  | 9kg, height 310mm, diameter 380mm, white and Red colour, Material: Plastic | Pc | 10 |  |  |
|  | Triplex  | Wooden 120cmx240cm | Pc | 6 |  |  |
|  | Trays  | Material: Paper, Capacity:30 Eggs, Colour: White | Pc | 10 |  |  |
|  | Disinfectants  | D4 | litres | 5 |  |  |
| Virocid  | litres | 5 |  |  |
| Cupacid  | litres | 5 |  |  |
| Farmer’s lime | Kg | 100 |  |  |

**Equipment and Materials to be delivered to the private sector**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **No.** | **Item Description** | **Item Specifications** | **Units** | **Quantity** | **Unit Price (Frw)** | **Total Price (Frw)** |
|  | Electronic weighing scale | 300 Kg | Pc | 1 |  |  |
|  | Electronic weighing scale | 5Kg & grams | PC | 1 |  |  |
|  | Automatic syringes | 60 mgs | Pc | 2 |  |  |
|  | Electric debeaker | Chicken debeaker | Pc | 1 |  |  |
|  | Digital thermometer | 3 units | Pc | 3 |  |  |
|  | Thermometer  | Thermometers for GH (6 units) with Min & Max | Pc | 6 |  |  |
|  | Moisture analyzer | Moisture analyzer for grain | Pc | 1 |  |  |

**NOTE:**

1. Kilimo Trust Rwanda, in a fair and transparent manner, will select companies that fulfill all requirements.
2. If necessary, interested bidders can visit the site any time before **28th February 2022**.
3. For items that need to be installed or assembled, the bidder should include installation and assembling cost in the bid.