**LOT 2: Supply of Meat Processing Equipment and Materials to the Integrated Polytechnic Regional College (IPRC) Musanze.**

*Bidders are expected to examine carefully and comply with all instructions and specifications.*

**Date: \_\_\_\_\_\_/\_\_\_\_\_\_/\_\_\_\_\_\_\_\_\_**

**Bidder Information**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | |  | |  | |  |
| Bidder’s Legal Name |  | | | | |  |
|  | | | | | | |
| TIN Number |  | | | | |  |
|  |  | | | | |  |
| Country/ies of Registration/Operation |  | | | | |  |
| |  | | --- | |  |   Bidder’s Authorized Representative | | | | | | |
|  |  | |  | |  |  |
| Title |  | | Telephone | |  |  |
|  | | | | | | |
| Email |  | | | | |  |
|  | | | | | | |

**Descriptions and Specifications of required Meat Processing Equipment and Materials to be supplied to IPRC Musanze.**

| **No.** | **Item Description** | **Item Specifications** | **Units** | **Quantity** | **Unit Price (Frw)** | **Total Price (Frw)** |
| --- | --- | --- | --- | --- | --- | --- |
|  | Pork stunning gun |  | Pcs | 1 |  |  |
|  | Meat tenderizer | Automatic electric High speed meat tenderizer machine  Voltage: 220V | Pcs | 5 |  |  |
|  | Electrical Meat slicer | Fresh meat slicing and initial processing, with adjustable sizes and shapes. | Pcs | 1 |  |  |
|  | Stuffer (stuffing machine) | Capacity 25 L max; Power 230 V; Dimensions 720 x 570 x 1380 mm; with differents size filling funnels | Pcs | 1 |  |  |
|  | Meat Smoker | Electric meat smoker; 380 V; Dimensions approx 75 x 130 x 65 cm;  With adjustable temperature settings | Pcs | 1 |  |  |
|  | Hamburger press machine | Manual burger making machine  Packing size: 520\*320\*396mm | Pcs | 1 |  |  |
|  | Hygrometer | Mini LCD Digital Thermometer Hygrometer Thermostat Indoor Convenient Temperature Sensor Humidity Meter Gauge Instruments Probe, button battery, heat resistant | Pcs | 5 |  |  |
|  | Cleaver knives | Knives with plastic handles. Stainless steel blades | Pcs | 12 |  |  |
|  | Butcher knives | Knives with plastic handles. Stainless steel blades | Pcs | 12 |  |  |
|  | Boning knife | Knives with plastic handles. Stainless steel blades | Pcs | 12 |  |  |
|  | Bowl for minced meat | Stainless steel (10 L, 5l,) with handles | Pcs | 5 |  |  |
|  | Hooks | Stainless Steel S Hooks with Sharp Tip Utensil Meat Hanger,Size: Approx. 12.5x5 cm | Pcs | 10 |  |  |
|  | Analytical Balance, ug, 0/001-0.01 | Electric balance  Capacity: 0.1gr- 5kg | Pcs | 2 |  |  |
|  | Sodium Nitrite | white crystalline solid,melting point of 308 degree celcius,density of 2.26 g/ml,bottle of 500 grs,bottle.  Shelflife: at least 2 years from supply | Kg | 5 |  |  |
|  | M. glutamate | colorless or waxy white,powder or cristals, at least 2 years from supply | Kg | 5 |  |  |
|  | Phosphate | colorless or waxy white,powder or cristals, at least 2 years from supply | Kg | 5 |  |  |
|  | Cooking oil | Vegetable oil, with 2 years shelflife from supplying date | L | 400 |  |  |
|  | Garlic powder | Powdered, packaged in small bottles (100g or less) with at least 2 years from supply | Bottle | 90 |  |  |
|  | Black pepper powder | Powdered, packaged in small bottles (100g or less) with at least 2 years from supply | Bottles | 30 |  |  |
|  | White pepper powder | Powdered, packaged in small bottles (100g or less) with at least 2 years from supply | Bottles | 30 |  |  |
|  | Artificial casings | Edible halal Collagen materials, with different sizes: 250gr, 500gr and 1000g | Kg | 60 |  |  |
|  | Papain powder | Enzyme for meat processing,  Powder form with a shelf-life of least 2 years from supply | Kg | 4 |  |  |
|  | Hydrogen peroxide | colorless or waxy white, powder or cristals, at least 2 years from supply | L | 20 |  |  |
|  | Sodium Hypochlorite | Disinfecting agent,  Concentration1-4%concentration with dilution direction  **Shelf-life:** 2 years from supplying date | L | 60 |  |  |
|  | Chlorine | Concentrated with dilution direction  With a long shelf-life | L | 20 |  |  |

**NOTE:**

1. Kilimo Trust Rwanda, in a fair and transparent manner, will select companies that fulfill all requirements.
2. If necessary, interested bidders can visit the site any time before **28th February 2022**.
3. For items that need to be installed or assembled, the bidder should include installation and assembling cost in the bid.