**LOT 9: Supply of Equipment and Materials for Animal Feed Production to the Department of Veterinary Technology at the Integrated Polytechnic Regional College (IPRC) Huye.**

*Bidders are expected to examine carefully and comply with all instructions and specifications.*

**Date: \_\_\_\_\_\_/\_\_\_\_\_\_/\_\_\_\_\_\_\_\_\_**

**Bidder Information**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | |  | |  | |  |
| Bidder’s Legal Name |  | | | | |  |
|  | | | | | | |
| TIN Number |  | | | | |  |
|  |  | | | | |  |
| Country/ies of Registration/Operation |  | | | | |  |
| |  | | --- | |  |   Bidder’s Authorized Representative | | | | | | |
|  |  | |  | |  |  |
| Title |  | | Telephone | |  |  |
|  | | | | | | |
| Email |  | | | | |  |
|  | | | | | | |

**Descriptions and Specifications of required Equipment and Materials to be supplied to the Department of Veterinary Technology at the Integrated Polytechnic Regional College (IPRC) Huye.**

| **No.** | **Item Description** | **Item Specifications** | **Units** | **Quantity** | **Unit Price (Frw)** | **Total Price (Frw)** |
| --- | --- | --- | --- | --- | --- | --- |
|  | Mixers (Vertical) | Name: vertical type animal feed mixer with crusher  Applicable material shape: powder  Condition: new  Processing techniques: crushing before mixing  Processing object: mixed feed  Type: mixing equipment  Suitable: manufacturing plant, farms and feed meal  Raw materials: corn, wheat, sorghum, beans  Warranty: 1year  Color: Green  Transport package: wooden box. | Pcs | 1 |  |  |
|  | Feed formulation software | Standard feed formulation software for example Win Feed, Feed solution interactive software for 30 users, identify feed ingredients and its nutrients values and formulate diet based on common ingredients.  Subscription per year | Pcs | 1 |  |  |
|  | Grinder Machine | Name: Animal feed grain grinder crusher mixer combined machine  Model no: CE,CO,BV  Condition new  Certification: CE,ISO 9001  Precision: Higher precision  Cylindrical grinder type: universal cylinder grinder  Automatic grade: Semi-automatic  Controlling mode: artificial  Abrasives : grinding wheel  Processing object: gear  Trademark: GMEC  Specification: 3 cubic | Pcs | 1 |  |  |
|  | Small Feed Pellet Machine | Product name: Animal Feed Pellet Plant  Applicable Industries: Farms  Condition: New  Brand Name: Smartech  Type: Feed Pellet Machine  Voltage: 380v, 50hz, 3phase  Dimension(L\*W\*H): referring to drawing  Weight: 100 kg  Warranty: 2 years  Warranty: 1 Year  Core Components: Gear, Bearing, Engine  Max. Capacity: 50-1000kgs  Raw material: Wheat, Bran | Pcs | 1 |  |  |
|  | Feed Pellet Cooler | Applicable Industries: Farms  Condition: New  Brand Name: Tongfu  Type: Cooling Machine  Voltage: 380V  Dimension(L\*W\*H):  2850\*2120\*2860 mm  Weight: 1580 kg  Warranty: 1 Year  Certification: CE  Application: Pellet Cooling Processing  Volume: 4 cbms  Capacity: 10 t/h  Cooling Time: Less Than 10-15mins  Power: 1.5 kw  Accessory 1: Cyclone  Accessory 2: Air Fan  Accessory 3: Air Lock | Pcs | 1 |  |  |
|  | Feed packaging machine (Weighing range (25-50kg/bag) | Type: Multi-Function Packaging Machine  Applicable Industries: Farms  Condition: New  Function: FILLING, Sealing  Packaging Type: Bags  Automatic Grade: Semi-automatic  Voltage: 380V/50HZ  Brand Name: Fuliang  Dimension(L\*W\*H): 3000\*1200\*2100mm  Warranty: 1 Year  Production Capacity: 20bag/min,  Product name: High Quality powder packing machine  Weighing Range: 5-70kg  Machine material: Stainless Steel  Application Materials: feed, fertilizer, grain,sugar, bean, rice | Pcs | 1 |  |  |
|  | Stainless Steel Cooking Vessel (Capacity: 50 Litres) | Condition: New  Warranty of core components: 1 Year  Core Components:  Engine  Brand Name: GuoLong  Type: Cooking Equipment  Warranty: 1 Year  Machinery Capacity: 50L  Machinery Function: Cooking | Pcs | 1 |  |  |

**NOTE:**

1. Kilimo Trust Rwanda, in a fair and transparent manner, will select companies that fulfill all requirements.
2. If necessary, interested bidders can visit the site any time before **28th February 2022**.
3. For items that need to be installed or assembled, the bidder should include installation and assembling cost in the bid.