**LOT 9: Supply of Equipment and Materials for Animal Feed Production to the Department of Veterinary Technology at the Integrated Polytechnic Regional College (IPRC) Huye.**

*Bidders are expected to examine carefully and comply with all instructions and specifications.*

**Date: \_\_\_\_\_\_/\_\_\_\_\_\_/\_\_\_\_\_\_\_\_\_**

**Bidder Information**

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
| Bidder’s Legal Name |  |  |
|  |
| TIN Number |  |  |
|  |  |  |
| Country/ies of Registration/Operation |  |  |
|

|  |
| --- |
|  |

Bidder’s Authorized Representative |
|  |  |  |  |  |
| Title |  |  Telephone |  |  |
|  |
| Email |  |  |
|  |

**Descriptions and Specifications of required Equipment and Materials to be supplied to the Department of Veterinary Technology at the Integrated Polytechnic Regional College (IPRC) Huye.**

| **No.** | **Item Description** | **Item Specifications** | **Units** | **Quantity** | **Unit Price (Frw)** | **Total Price (Frw)** |
| --- | --- | --- | --- | --- | --- | --- |
|  | Mixers (Vertical) | Name: vertical type animal feed mixer with crusherApplicable material shape: powderCondition: newProcessing techniques: crushing before mixingProcessing object: mixed feedType: mixing equipmentSuitable: manufacturing plant, farms and feed mealRaw materials: corn, wheat, sorghum, beansWarranty: 1yearColor: GreenTransport package: wooden box. |  Pcs | 1 |  |  |
|  | Feed formulation software | Standard feed formulation software for example Win Feed, Feed solution interactive software for 30 users, identify feed ingredients and its nutrients values and formulate diet based on common ingredients.Subscription per year | Pcs | 1 |  |  |
|  | Grinder Machine | Name: Animal feed grain grinder crusher mixer combined machineModel no: CE,CO,BVCondition newCertification: CE,ISO 9001Precision: Higher precisionCylindrical grinder type: universal cylinder grinderAutomatic grade: Semi-automaticControlling mode: artificialAbrasives : grinding wheelProcessing object: gearTrademark: GMECSpecification: 3 cubic  |  Pcs | 1 |  |  |
|  | Small Feed Pellet Machine | Product name: Animal Feed Pellet PlantApplicable Industries: FarmsCondition: NewBrand Name: SmartechType: Feed Pellet MachineVoltage: 380v, 50hz, 3phaseDimension(L\*W\*H): referring to drawingWeight: 100 kgWarranty: 2 yearsWarranty: 1 YearCore Components: Gear, Bearing, EngineMax. Capacity: 50-1000kgsRaw material: Wheat, Bran  | Pcs  | 1 |  |  |
|  | Feed Pellet Cooler | Applicable Industries: FarmsCondition: NewBrand Name: TongfuType: Cooling MachineVoltage: 380VDimension(L\*W\*H):2850\*2120\*2860 mmWeight: 1580 kgWarranty: 1 YearCertification: CEApplication: Pellet Cooling ProcessingVolume: 4 cbmsCapacity: 10 t/hCooling Time: Less Than 10-15minsPower: 1.5 kwAccessory 1: CycloneAccessory 2: Air FanAccessory 3: Air Lock  | Pcs  | 1 |  |  |
|  | Feed packaging machine (Weighing range (25-50kg/bag) | Type: Multi-Function Packaging MachineApplicable Industries: FarmsCondition: NewFunction: FILLING, SealingPackaging Type: BagsAutomatic Grade: Semi-automaticVoltage: 380V/50HZBrand Name: FuliangDimension(L\*W\*H): 3000\*1200\*2100mmWarranty: 1 YearProduction Capacity: 20bag/min,Product name: High Quality powder packing machineWeighing Range: 5-70kgMachine material: Stainless SteelApplication Materials: feed, fertilizer, grain,sugar, bean, rice | Pcs  | 1 |  |  |
|  | Stainless Steel Cooking Vessel (Capacity: 50 Litres) | Condition: NewWarranty of core components: 1 YearCore Components:EngineBrand Name: GuoLongType: Cooking EquipmentWarranty: 1 YearMachinery Capacity: 50LMachinery Function: Cooking  | Pcs  | 1 |  |  |

**NOTE:**

1. Kilimo Trust Rwanda, in a fair and transparent manner, will select companies that fulfill all requirements.
2. If necessary, interested bidders can visit the site any time before **28th February 2022**.
3. For items that need to be installed or assembled, the bidder should include installation and assembling cost in the bid.